#include <avr/io.h>

#define *F\_CPU* 16000000

#include <util/delay.h>

#include <stdlib.h>

int main()

{

DDRD = 0XFF;

while(1)

{

PORTD = 0x02;

*\_delay\_ms*(200);

PORTD = 0x01;

*\_delay\_ms*(200);

}

}